**LED Creative Display Product Categories**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Personalized** **LED** **display** | | | | | | | | | | | | | | | | | | |
| **LED** **Badge** | | | | **LED** **Hat** | | | | | | | | **LED** **Collar** | | **LED** **Bottle** | | | **LED** **Mask** | |
|  | |  | | WEL | |  | | 欢迎 | |  | |  | |  |  | | 1 | |
| **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | | **item#** | **color** |
| B1248 | red | B1248BL | red | M536  (English) | Monodhrome | M1248A | Monochrome | M1248B internal | Monochro me | M1632 | RGB | C1248 | Monochrome | W1248 | Monochrome | | M1248D | Monochrome |
| blue | blue |
| green | green | pink | pink | pink | pink | pink | | pink |
| white | white |
| pink | pink | multi color | external | multi color | multi color | multi color | multi color | | multi color |
| Purple | multi single color | M1632D | RGB |
| size:93\*30\*6MM  pixels:44\*11 dots  communication:USB-PC  Power:Lithium battery installation:pin/magnet weight:50G/set  box size:11\*7\*2CM  100pcs carton size:39\*25\*16 CM | | size:93\*30\*6MM  pixels:48\*12 dots  communication:bluetooth APP power:lithium battery  installation:pin/magnet weight:50G/set  box size:11\*7\*2CM  100pcs carton size:39\*25\*16 CM | | size:free /adjustable  pixels:48\*12 dots  communication:bluetooth APP  power:lithium battery  installation:wearable  weight:145G/set  packing size:24\*23\*14CM  10pcs:39\*25\*16CM 25pcs 62\*25\*19CM  100pcs:69\*50\*32CM | | size:free /adjustable  pixels:48\*12 dots  communication:bluetooth APP  power:lithium battery  Installation:wearable  weight:160G/set  packing sire:24\*23\*14CM  10pcs:39\*25\*1CM  25pcs 62\*25\*19 CM  100pcs:69\*50\*32 CM | | size:free /adjustable  pixels:48\*12 dots  communication:bluetooth APP  power:lithium battery  installation:wearable  weight:160G/set  packing size:24\*23\*14CM  10pcs:39\*25\*16 CM  25pcs:62\*25\*19 CM  100pcs:69\*50\*32 CM | | size:free /adjustable  pixels:32\*16 dots  communication:bluetooth APP power:lithium battery  installation:wearable weight:180G/set  packing size:24\*23\*14CM  10pcs:39\*25\*16CM 25pcs:62\*25\*19CM 100pcs:69\*50\*32CM | | size:free /adjustable  pixels:48\*12 dots  communication:bluetooth APP  power:lithium battery  installation:wearable  weight:105G/set  packing size:48\*8\*6 CM | | size:free /adjustable  pixes:48\*12 dots  communication:bluetooth APP  power:lithium battery installation:wearable weight:55G/set  packing size:26\*12\*9 CM | | | size:free /adjustable  picels:48\*12 dots/32\*16 dots  communication:bluetooth APP  power:lithium battery installation:wearable weight:55G/set  packing size:26\*15\*5 CM | |
| **LED** **powerbank** | | **LED** **fannybag** | | | | | | **LED** **Backpack** | | | | **LED** **VEST** | | **LED** **T-SHIRT** | | | **LED** **frame** **screen** | |
| 移动电源 | |  | |  | | )ap | |  | |  | |  | |  | |  |  | |
| **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | **item#** | **color** | | **item#** | **color** |
| BLP801 | Monochrome | B102 | RGB | B103 | RGB | B104 | RGB | B201  (Tech Cloth) | RGB FUL  COLOR | B301  (PU leather) | RGB FULL  COLOR | T6464-1  Single-sided | full color | T1632 | RGB | | D3-6464 | RGB |
| pink | T6464-2  Double Sided | full color | D3-64128 | RGB |
| multi color |
| Size:158\*75\*15 MM Display  dot matric 48\*12 dots  transmission mode:Bluetooth  APP  Powersupply mode:lithium battery  Installation:WearableWeight 400G/set  Package size:26\*12\*4CM | | Size:176\*76 MM  Display lattice:32\*16 dots  Transmission mode:Bluetooth APP  Power supply mode:lithium battery Installatione Wearable  Weight 450G/set  Package size:31\*29\*7 CM | | Size:176\*76 MM  Display dot matrixc:32\*16 dots  transmission mode:Bluetooth APP Power supply mode.lithium battery Installation:Wearable  Weight:450G/set  Package size:31\*29\*7 CM | | Size:180\*180MM Display dot matric 64\*64 dots  transmission mode:Bluetooth APP Powersupply mode:lithium  battery  Installation:Wearable Weight:500G/set  Packagesize:31\*29\*70M | | Size:260\*260 MM Display dot matric 64\*64 dots  transmission moder Bluetooth APP  Power supply mode:power bank Installation:Wearable  Weight:1600 G/set  Package size:48\*20\*36 CM | | Size:260\*260 MM  Display dot matribc:64\*64 dots  transmission mode:Bluetooth APP  Power supply mode:power bank Installation:Wearable  Weight:1600 G/set  Package size:48\*20\*36 CM  10pcs Size:47\*66\*64 CM | | Size:260\*260 MM  Display dot matrix:48\*12 dots  transmission mode:Bluetooth APP  Power supply mode power bank  Installation:Wearable Weight:140G/set  Package size:32\*29\*8 CM | | Size:200\*260MM  Display dotmatrixc 32\*16 dots transmissionmode:BluetoothAPP Power supply mode:power bank nstallation:Wearable  Weight:120G/set  Package size:32\*29\*8CM | | | Size:195\*195\*20MM 387\*195\*20MM  Display dotmatrix:128\*64 dot  Transmission mode: WIFI  communication  Power supply moder USB cable Installation method:stand  Weight:950G/set | |
| Note: Red,yellow,blue.green,white are available for Monochrome color  Standard configuration: one led screen,one USB communication,one manual,neutral carton packaging. | | | | | | | | | | | | | | | | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **RGB color ultra-thin flexible LED display** | | | | | | | | | | | | |
| **Picture** | **Model** | **LED** **color** | **Border** | **Pixel** | **screen** **size** | **communication** | **Power** | **Color** **box** **size** | **Weight** | **Outer** **box** **size** | **qty/box** | **G.W./box** |
| 只吧  LL  B AUTY  B AUT¹Q | S3232 | RGB | PU | 32\*32 dots | 230\*187mm | Bluetooth APP | 5V/12V | 23\*11\*10CM | 300g | 60\*50\*45CM | 40 | 12kg |
| S1632 | RGB | PU | 16\*32 dots | 148\*90 mm | Bluetooth APP | 5V/12V | 13.5\*11\*10CM | 250g | 60\*45\*25CM | 30 | 7.5kg |
| S1664 | RGB | PU | 16\*64 dots | 390\*107 mm | Bluetooth APP | 5V/12V | 13.5\*11\*10CM | 300g | 60\*45\*25CM | 30 | 9kg |
| S1696 | RGB | PU | 16\*96 dots | 672\*122 mm | Bluetooth APP | 5V/12V | 13.5\*11\*10CM | 400g | 60\*45\*25CM | 30 | 12kg |
| S3264 | RGB | PU | 32\*64 dots | 390\*187 mm | Bluetooth APP | 5V/12V | 23\*11\*10CM | 400g | 60\*50\*45CM | 40 | 16kg |
| S3296 | RGB | PU | 32\*96 dots | 672\*218 mm | Bluetooth APP | 5V/12V | 23\*11\*10CM | 500g | 60\*50\*45CM | 40 | 20kg |
| P1696 | RGB | PU | 16\*96 dots | 705\*130 mm | Bluetooth APP | 5V/12V | 30\*25\*13.5cm | 450g | 67\*48\*30cm | 30 | 13kg |
| P32128  (1921) | RGB | PU | 32\*128 dots | 705\*220 mm | Bluetooth APP | 5V/12V | 30\*25\*13.5cm | 800g | 67\*48\*30cm | 20 | 15kg |
| F1664 | RGB | PU | 16\*64 dots | 276\*90 mm | Bluetooth APP | 5V/12V | 13.5\*11\*10CM | 250g | 60\*45\*25CM | 30 | 7.5kg |
| F16128 | RGB | PU | 16\*128 dots | 532\*90 mm | Bluetooth APP | 5V/12V | 13.5\*11\*11CM | 500g | 60\*45\*25CM | 30 | 15kg |
| F16192 | RGB | PU | 16\*192 dots | 788\*90 mm | Bluetooth APP | 5V/12V | 13.5\*11\*12CM | 750g | 60\*45\*25CM | 30 | 22.5kg |
| F16256 | RGB | PU | 16\*256 dots | 1044\*90 mm | Bluetooth APP | 5V/12V | 13.5\*11\*13CM | 1000g | 60\*45\*25CM | 30 | 30kg |
| F16320 | RGB | PU | 16\*320 dots | 1300\*90 mm | WIFI | 5V/12V | 13.5\*11\*14CM | 1250g | 60\*45\*25CM | 30 | 37.5kg |
| F16384 | RGB | PU | 16\*384 dots | 1560\*90 mm | WIFI | 5V/12V | 13.5\*11\*15CM | 1500g | 60\*45\*25CM | 30 | 45kg |
| F3264 | RGB | PU | 32\*64 dots | 260\*150 mm | Bluetooth APP | 5V/12V | 16\*11\*10CM | 350g | 60\*35\*25CM | 20 | 7kg |
| F32128 | RGB | PU | 32\*128 dots | 500\*150 mm | Bluetooth APP | 5V/12V | 16\*11\*10CM | 700g | 60\*35\*25CM | 20 | 14kg |
| F32192 | RGB | PU | 32\*192 dots | 740\*150 mm | WIFI | 5V/12V | 16\*11\*10CM | 1050g | 60\*35\*25CM | 20 | 21kg |
| F32256 | RGB | PU | 32\*256 dots | 980\*150 mm | WIFI | 5V/12V | 16\*11\*10CM | 1400g | 60\*35\*25CM | 20 | 28kg |
| F32320 | RGB | PUI | 32\*320 dots | 1220\*150 mm | WIFI | 5V/12V | 16\*11\*10CM | 1750g | 60\*35\*25CM | 20 | 35kg |
| F32384 | RGB | PU | 32\*384 dots | 1460\*150 mm | WIFI | 5V/12V | 16\*11\*10CM | 2100g | 60\*35\*25CM | 20 | 42kg |


|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Ultra-thin LED Display Products** | | | | | | | | | | | | |
| **Product** **images** | **Model** | **Color** | **Border** | **Pixel** | **Screen** **size** | **ommunication** | **Power** | **Color** **boxsize** | **Weight** | **Outer** **box** **size** | **qty/ctn** | **Weight** |
|  | K1648 | Monochrome | Aluminum frame | 48\*16 points | 260\*95\*15 mm | Bluetooth APP | 5V/12V | 360\*130\*35 mm | 0.45KG | 50\*44\*32CM | 20 | 11kg |
| K1664 | Monochrome | Aluminum frame | 64\*16 points | 340\*95\*15 mm | Bluetooth APP | 5V/12V | 440\*130\*35 mm | 0.6KG | 50\*44\*32CM | 20 | 14kg |
| K1680 | Monochrome | Aluminum frame | 80\*16 points | 410\*95\*15 mm | Bluetooth APP | 5V/12V | 510\*130\*35 mm | 0.7KG | 56\*49\*32CM | 20 | 16kg |
| K1696 | Monochrome | Aluminum frame | 96\*16 points | 500\*95\*15 mm | Bluetooth APP | 5V/12V | 595\*130\*35 mm | 0.7KG | 69\*50\*32CM | 20 | 16kg |
| K16128 | Monochrome | Aluminum frame | 128\*16 points | 660\*95\*15 mm | Bluetooth APP | 5V/12V | 770\*130\*35 mm | 1.2KG | 85\*17\*12CM | 2 | 2.6kg |
| K16160 | Monochrome | Aluminum frame | 160\*16 points | 820\*95\*15 mm | Bluetooth APP | 5V/12V | 925\*130\*35 mm | 1.35KG | 107\*17\*12CM | 2 | 2.9kg |
| K16192 | Monochrome | Aluminum frame | 192\*16 points | 980\*95\*15 mm | Bluetooth APP | 5V/12V | 1080\*130\*35 mm | 1.55KG | 114\*31\*38CM | 20 | 32.5kg |
| K16224 | Monochrome | Aluminum frame | 224\*16 points | 1140\*95\*15 mm | Bluetooth APP | 5V/12V | 1240\*130\*35 mm | 1.75KG | 121\*31\*38CM | 20 | 36kg |
|  | K16256 | Monochrome | Aluminum frame | 256\*16 points | 1300\*95\*15 mm | Bluetooth APP | 5V/12V | 1400\*135\*35 mm | 1.95KG | 138\*143\*38CM | 10 | 40.5kg |
| K16288 | Monochrome | Aluminum frame | 288\*16 points | 1460\*95\*15 mm | Bluetooth APP | 5V/12V | 1560\*135\*35 mm | 2.15KG | 153\*143\*38CM | 10 | 23kg |
| K16320 | Monochrome | Aluminum frame | 320\*16 points | 1620\*95\*15 mm | Bluetooth APP | 5V/12V | 1720\*135\*35 mm | 2.35KG | 169\*143\*38CM | 10 | 24.8kg |
| K1664 | RGB | Aluminum frame | 64\*16 points | 340\*95\*15 mm | Bluetooth APP | 5V/12V | 440\*130\*35 mm | 0.6KG | 50\*44\*32CM | 20 | 11kg |
| K1696 | RGB | Aluminum frame | 96\*16 points | 500\*95\*15 mm | Bluetooth APP | 5V/12V | 510\*130\*35 mm | 0.7KG | 50\*44\*32CM | 20 | 14kg |
|  | K16128 | RGB | Aluminum frame | 128\*16 points | 660\*95\*15 mm | Bluetooth APP | 5V/12V | 595\*130\*35 mm | 1.2KG | 56\*49\*32CM | 20 | 16kg |
| K16160 | RGB | Aluminum frame | 160\*16 points | 820\*95\*15 mm | Bluetooth APP | 5V/12V | 770\*130\*35 mm | 1.35KG | 69\*50\*32CM | 20 | 16kg |
| K16192 | RGB | Aluminum frame | 192\*16 points | 980\*95\*15 mm | Bluetooth APP | 5V/12V | 925\*130\*35 mm | 1.55KG | 114\*31\*38CM | 20 | 32.5kg |
| K16224 | RGB | Aluminum frame | 224\*16 points | 1140\*95\*15 mm | Bluetooth APP | 5V/12V | 1080\*130\*35 mm | 1.75KG | 121\*31\*38CM | 20 | 36kg |
|  | K16256 | RGB | Aluminum frame | 256\*16 points | 1300\*95\*15 mm | Bluetooth APP | 5V/12V | 1240\*130\*35 mm | 1.95KG | 138\*143\*38CM | 10 | 40.5kg |
| K16288 | RGB | Aluminum frame | 288\*16 points | 1460\*95\*15 mm | Bluetooth APP | 5V/12V | 1400\*135\*35 mm | 2.15KG | 153\*143\*38CM | 10 | 23kg |
| K16320 | RGB | Aluminum frame | 320\*16 points | 1620\*95\*15 mm | Bluetooth APP | 5V/12V | 1560\*135\*35 mm | 2.35KG | 169\*143\*38CM | 10 | 24.8kg |
| 告条屏  线发送车载 EDMHDSP | K2448 | RGB | Aluminum frame | 48\*24 points | 260\*156\*22 mm | Bluetooth APP | 5V/12V | 1720\*135\*35 mm | 0.6KG | 33\*41\*58CM | 20 | 13kg |
| K2496 | RGB | Aluminum frame | 96\*24 points | 510\*156\*22 mm | Bluetooth APP | 5V/12V | 645\*165\*50 mm | 1KG | 58\*41\*58CM | 20 | 21kg |
| K24144 | RGB | Aluminum frame | 144\*24 points | 750\*156\*22 mm | Bluetooth APP | 5V/12V | 910\*165\*50 mm | 1.6KG | 82\*41\*58CM | 20 | 33kg |
| K24192 | RGB | Aluminum frame | 192\*24 points | 990\*156\*22 mm | Bluetooth APP | 5V/12V | 1040\*165\*50 mm | 2.2KG | 105\*22\*58CM | 10 | 23kg |
| K24240 | RGB | Aluminum frame | 240\*24 points | 1130\*156\*22 mm | Bluetooth APP | 5V/12V | 1280\*165\*50 mm | 2.9KG | 118\*22\*58CM | 10 | 30kg |
|  | K24288 | RGB | Aluminum frame | 288\*24 points | 1470\*156\*22 mm | Bluetooth APP | 5V/12V | 1620\*165\*50 mm | 3.2KG | 153\*22\*58CM | 10 | 33kg |



|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Vehicle** **LED** **Display** | | | | | | | | | | | | | | | | | | |
| **Mini** **LED** **car** **screen(European** **and** **American** **remote** **control** **version)** | | | | | | | | | | | | | | | | | | |
|  | | |  | | | |  | | | |  | | | |  | | | |
| **Model** | **Screen** **size** **MM** | **Color** | **Model** | **Screen** **size** **MM** | **Color** | **Color** | **Model** | **Screen** **size** **MM** | **Color** | **Color** | **Model** | **Screen** **size** **MM** | **Color** | **Color** | **Model** | S**creen** **size** **MM** | **Color** | **Color** |
| Z723 | 133\*33\*7 | Red | Z740 | 340\*50\*10 | Red | Red | Z741 | 230\*50\*10 | Red | Red | B741 | 288\*80\*15 | Red | Red | D750 | 433\*95\*66 | Red | Red |
| Blue | Blue | Blue | Blue | Blue | Blue | Blue | Blue | Blue |
| White | White | White | White | White | White | White | White | White |
| Pink | Pink | Pink | Pink | Pink | Pink | Pink | Pink | Pink |
| Display lattice:23\*7 dots  Transmission mode:remote control input  Power supply mode:12 V red and black wire  Installation method:suction cup(standard)  Packagesize:20\*14 CM | | | Display lattice:40\*7 dots  Transmission mode:remote control input  Power supply mode:12V cigarette lighter with car cable  Installation method:suction cup(standard)  Color box size:32\*6\*14 CM | | | | Display lattice:41\*7 dots  Transmission mode:remote control input  Power supply mode:12V cigarette lighter withcar cable  Installation method:suction cup (standard)  Color box size:28\*6\*7 CM | | | | Display lattice:41\*7 dots  Transmission mode:USB+remote control input  Power supply mode:12V cigarette lighter with car cable  Installation method:suction cup (standard)  Color boxsize:338\*100\*30 MM | | | | Display dot matrix:50\*7 dots  Transmission mode:remote control input  Power supply mode:12V cigarette lighter with car cable  Installation method:double-sided adhesive tape (standard) | | | |
| **Mini** **LED** **car** **screen(multi-language** **app** **version**) | | | | | | | | | | | **Rear** **window** **LED** **car** **display** | | | | | | | |
|  | | |  | | | | D1272 BL | | | | **彩** **色** **车** **扩** **告** **屏** | | | | 大 Insp | | | |
| **Model** | S**creen** **size** **MM** | **Color** | **Model** | | **Screen** **size** **MM** | **Color** | | **Model** | S**creen** **size** **MM** | **Color** | | **Model** | **Screen** **size** **MM** | **Color** | | **Model** | **Screen** **size** **MM** | **Color** | |
| Z1272 | 230\*50\*10 | Red | X1272 | 360\*90\*15 | RGB | | D1272 | 433\*95\*66 | Color | | K1664 | 340\*95\*15 | RGB | | K2448 | 260\*160\*22 | RGB | |
| Blue | K1696 | 500\*95\*15 | RGB | | K2496 | 510\*160\*22 | RGB | |
| White | K1612 | 660\*95\*15 | RGB | | K24144 | 750\*160\*22 | RGB | |
| Pink | K1616 | 820\*95\*15 | RGB | | K24192 | 990\*156\*22 | RGB | |
| Display lattice:72\*12 dots  Transmission mode:APP input  Power supply mode:12V cigarette lighter with car cable  Installation method:suction cup (standard)  Color box size:28\*6\*7 CM | | | Display lattice:72\*12 dots  Transmission mode:mobile phoneAPP transmission  Power supply mode:12Vcigarette lighter with car cable  Installation method:suction cup(standard)  Color box size:51\*13\*35 CM | | | | Display lattice:72\*12 dots  Transmission mode:mobile phone APP transmission  Power supply mode:12V cigarette lighter with car cable  Installation method:double-sided adhesive tape (standard)  Color box size:483\*125\*100MM | | | | Display dot matrix.64/96/128/160\*16 dots  Transmission mode:WIFI communication Power supply mode:adapter  Installation method:hanging chain and suction  cup  Weight:600G/700G/1200G/1350G/set | | | | Display dot matrix:48/96/144/192\*24 dots  Transmission mode:WIFI communication Power supply mode:adapter  Installation method:hanging chain and suction cup Weight:600G/1000G/1600G/2200G/set | | | |
| **LED** **expression** **screen** | | | | | | | | | | | **Intelligent** **tail** **lights** **for** **bicycles** **and** **electric** **vehicles** | | | | | | | |
|  | | |  | | | |  | | | | **《** | | | |  | | | |
| **Model** | **Screen** **size** **MM** | **Color** | **Model** | **Screen** **size** **MM** | **Color** | | **Model** S**creen** **size** **MM** | | **Color** | | **Model** | **Screen** **size** **MM** | **Color** | | **Model** | **Screen** **size** **MM** | **Color** | |
| P225 | Diameter 225 MM | RGB | P3201 | 150\*150\*22 | RGB | | P2541 185\*185\*22 | | RGB | | BK1248 | 225\*5\*15 | RGB | | BK536 | 195\*3\*15 | Monoch rome | |
| P3202 | 180\*180\*22 | RGB | | P3402 215\*215\*22 | | RGB | |
| P3203 | 210\*210\*22 | RGB | | P4403 280\*280\*22 | | RGB | |
| Display dot matrix:48\*48 dots  Transmission mode:bluetooth APP  Power supply mode:USB cable  Installation method:suction cup Package size:25\*25\*8cm  Weight:750G/set | | | Display dot matrix:32\*32 dots  Transmission mode:WIFI communication  Power supply mode:USB cable  nstallation method:suctioncup  Package size:26\*24\*7 CM Weight 650G/set | | | | Display dot matrix:64\*64 dots  Transmission mode:WIFI communication  Power supply mode:USB cable  Installation method:suction cup  Package size:26\*24\*7 CM Weight 650G/set | | | | Displaydot matrix48\*12 dots  Transmission mode:bluetooth APP Power supply mode:USB cable  Installation method:suction cup Package size:26\*24\*7 CM  Weight:650G/set | | | | Display dot matrix:36\*5 dots  Transmission mode:bluetooth APP  Powersupply mode:USB cable  Installation method:suction cup  Package size:26\*24\*7 CM Weight:650G/set | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Desktop LED Display Products** | | | | | | | | | | | | | | | | | | | |
| **LED** **desktop** **screen(dot** **matrix** **series)** | | | | | | | | **LED** **Desktop** **Screen(SMT** **Series)** | | | | | | | | | | | |
| **C1648** | | **C1664** | | **C1696** | | **C16128** | | **B1664** | | **B1696** | | **B16128** | | **S1664** | | **S1696** | | **S16128** | |
|  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |
| **Color** |  | **Color** | **Unit** **Price** | Color | **Unit** **Price** | Colot | Unit Price | Color | **Unit** **Price** | Color | **Unit** **Price** | Color | **Unit** **Price** | **Color** | **Unit** **Price** | **Color** | **Unit** **Price** | **Color** | **Unit** **Price** |
| Red |  | Red | USs207 | Red | US$26.92 | Red | US$33.08 | Red | US$13.08 | Red | US$16.62 | Red | US$19.38 | Red | US$20.92 | Red | US$24.62 | Red | US$27.69 |
| Yellow |  | Yellow | US$23.85 | Yellow | US$33.08 | Yellow | US$35.08 | Blue | US$13.85 | Blue | US$17.69 | Blue | USs2077 | Blue | US$24.31 | Blue | US$28.15 | Blue | US$31.54 |
| Blue |  | Blue | US$33.08 | Blue | US$45.54 | Blue | US$55.08 | Green | US$14.62 | Green | US$20.00 | Green | US$22.77 | Molow | US$24.31 | yellow | US$28 | y ow | US$31.54 |
| Green |  | Green | US$40.77 | Green | US$47.69 | Green | US$56.15 | White | US$14.62 | White | US$20.00 | White | US$22.77 | Green | US$25.38 | Green | US$30.00 | Green | US$34.62 |
| RGY |  | RGY | US$23.85 | RGY | uss30.46 | RGY | US536.15 | Yellow | US$14.62 | Yellow | US$20.00 | Yellow | US$22.77 | White | US$25.38 | White | US$30.00 | White | US$34.62 |
| RBP |  | RBP | US$39.69 | RBP | US$51.54 | RBP | US$64.62 | Pink | US$20.77 | Pink | US$28.92 | Pink | US$33.85 | Pink | US$33.08 | Pink | US$42.31 | Pink | US$48.92 |
| Size:236\*110\*22 MM  Display dot matrix:48\*16 dots  fransmission mode:USB communication  Power supply mode Lithium battery | | Size:300\*110\*22 MM  Displaydotmatrix 64\*16 dots  Transmkssion mode uis  communication Power supply  node:Lithium battery  Package size:50\*44\*32 CM | | Size:430\*110\*22 MM  Display dotmatrix 96\*16 dots  Transmission mode:USB  communication Power supply mode:Lithium battery  Package size:56\*49\*32 CM | | Size:560\*110\*22 MM  Display dot matrix 128\*16 dots D ransmission mode:USB  ommunication Power supply mode:Lithium battery  Package size:69\*50\*32 CM | | Size:220\*76\*18 MM  isplay dot matrix 48\*12 dots Transmission mode:USB  communication Power supply  mode:lithium battery Package size:34\*8\*3cm | | Size:320\*76\*18MM  Displaydot matrix:72\*12 dots Transmission mode:USB  communication Power supply  mode:lithium battery  Package size:45\*14\*4.5cm | | Size:420\*76\*18 MM  Display dotmatric:96\*12 dots Transmission mode:USB  communication Power supply  mode:lithium battery  Package size:55\*14\*4.5cm | | Size:260\*112\*22 MM  Display dot matrix:48\*12 dots Transmission mode:USB  communication Power supply  mode:lithium battery  Single size:50\*44\*32 CM | | Size:360\*112\*22 MM  Display dot matrix:72\*12 dots  Transmission mode:USB  communication Power supply mode:lithium battery  Single size:56\*49\*32 CM | | Size:460\*112\*22 MM  Display dot matrixc 96\*12 dots Transmission mode:USB  communication Power supply mode:lithium battery  Single size:69\*50\*32 CM | |
| **LEDDesktop** **Screen(SMT** **Series)** | | | | | | | | **LED** **triangle** **conference** **screen** | | | | | | | | | | | |
| **CB1664** | | **CB1696** | | **CB16128** | | **CB16160** | | **BS1664** | | **BS1696** | | **BS16128** | | **KS1664** | | **KS3264** | | **KS32128** | |
|  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |
| **Color** | Red,Blue,Green,White,Yellow,Pink | **Color** | Red,Blue,Green,White,Yellow,Pink | **Color** | Red,Blue,Green,White,Yellow,Pink | **Color** | Red,Blue,Green,White,Yellow,Pink | **Color** | Red,White,Pink | **Color** | Red,White,Pink | **Color** | Red,White,Pink | **Color** | Monochrome,Color | **colo** | Color | **Color** | Color |
| Size:180\*54\*18MM  Display dot matrix:64\*16 dots  Transmission mode:USB communication  Power supply mode:lithium battery  Package size:36\*14\*4.5cm | | Size:260\*54\*18 MM  Display dot matrix 96\*16 dots  Transmission mode:USB ommunication  Power supply mode:lithium battery  Package size:45\*14\*4.5cm | | Size:340\*54\*18 MM  Display dot matrix:128\*16 dots  Transmission mode:USB communication  Powersupply mode:lithium battery  Package size:55\*14\*4.5cm | | Size:420\*54\*18 MM  Display dot matrix:160\*16 dots transmission mode:USB  communication  Power supply mode:lithium battery  Package size:55\*14\*4.5cm | | Size:220\*76\*85MM  Display dotmatrix:48\*12 dots  Transmission mode USB  Communication  Power suppy mode:Lithium battery  Package size:27\*15\*13 CM | | Size:320\*76\*85MM  Displaydot matrix:72\*12 dots  Transmission mode USB communication,  Power supply mode:Lithium battery  Package size:35\*14\*14 CM | | Size:420\*76\*85MM  Display dot matrix:96\*12 dots  Transmission mode:USB  communication  Power supply mode:lithium battery  Package size:68\*16\*5cm | | Size:340\*128\*128MM  Display dot matrix:64\*16 dots Transmission mode:WIFI+USB Power supply mode:Lithium battery  package size:35\*14\*14 CM | | Size:185\*128\*128MM  Displaydot matrix:64\*32 dots Transmission mode:WIFI+U disk  Power supply mode Lithium battery  Package size:55\*36\*26 CM | | Size:340\*128\*128MM  Display dot matrix:128\*32 dots spoints  Transmission mode:WIFI U disk  Power supply mode:  Lithium battery  Package size:55\*36\*26CM | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Personalized LED Display** | | | | | | | | | | | | | |
| **LED** **handheld** **sign** **(rechargeable)** | | | | | | | | | | | **LED** **community** **screen** | | |
| 一  周杰伦 | | | | 01 | | | **手举广告** **活动推** | | | |  | | |
| **Model** | **Screen** **size** | **Color** | | **Model** | **Screen** **size** | **Color** | **Model** | **Screen** **size** | **Color** | | **Model** | **Screen** **size** | **Color** |
|  |  |  |  | C1664 | 310\*110\*22mm | RGY |  |  |  |  |  |  | Single-sided |
| C6464 | 285\*285\*22mm | RGB | | C1696 | 430\*110\*22mm | RGY | P4-64128 | 150\*530\*22mm | RGB | | C64128 | 530\*270\*22mm | Two-sided |
| C16128 | 560\*110\*22mm | RGY | Other sizes are customized |
| Display dot matrix:64\*64 dots  Transmission mode:WIFI communication  Power supply mode:lithium battery Installation method:hand-held  Package size:32\*32\*6 CM | | | | Display lattice:128\*16 dots  Transmission mode:USB communication  Power supply mode:lithium battery Installation method:hand-held  Package size:69\*50\*32 CM | | | Display lattice:128\*64 dots  Transmission mode:WIFI communication  Power supply mode:lithium battery Installation method:hand-held  Package size:550\*180\*50MM | | | | Display lattice:128\*64 dots  Transmission mode:WIFI communication  Power supply mode:USB cable Installation method:hanging Package size:540\*280\*32 | | |
| **LED** **welcome** **screen** **board** | | | | **LED** **tobacco** **screen** | | | **LED** **magic** **cube** **screen** | | | | **Logo** **screen** | | |
| 欢迎光临 欢迎  LCOME | | | |  | | |  | | | |  | | |
| **Model** | **Screen** **size** | **Color** | | **Model** | **Screen** **size** | **Color** | **Model** | **Screen** **size** | **Color** | | **Model** | **Screen** **size** | **Color** |
| F475- 160128 | 800\*648\*50mm | Red | | B12432 | 1150\*28\*20mm | Red White  Pink | P25-128F5 | 320\*320\*320mm | full color | | P460 | 770\*110mm | full color |
| P3-128F5 | 384x384x384mm | full color | |
| RGY | | B12540 | 1430\*28\*20mm | Red White  Pink |
| P4-128F5 | 512x512x512mm | full color | |
| Display dot matrix:192\*256 dots  Transmission mode:U disk  Power supply mode:AC110V-220V  Installation method:floor stand (standard configuration)  Package size:650\*840\*100MM | | | | Display lattice:432\*12 o'clock/540\*12 o'clock  Transmission mode:U disk  Power supply mode:AC110V-220V Package size:1200\*50\*40MM | | | Display lattice:128\*128\*5 sides Transmission mode:WIFI  Power supply mode:AC110V-220V  Installation method:side hanging on four sides  Package size:350\*350\*350 MM | | | | Display dot matrix:128\*128 dots  Transmission mode:WIFI communication  Power supply mode:AC110V-220V  Installation method:side-mounted bracket Package size:820\*160MM | | |



**OEM Customized LED Display Product**

**Customized LED display upon request**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | |  | |  | |  | |
| ED手机壳L  LED童鞋LED children's shoes LED手环LED bracelet | | LED头盔LED helmet | **镇至3D挎包Shoulder** **bag**  镶至圆环Ring | |  | | 镇至发光话筒Microphon | | 镇至潮流板鞋Skate shoes |
| **镶至眼镜Glasses** | | **镶至衣服Clothing** | | 镶至手环Wristband |

8